Glossary
Glossary of aerospace manufacturing and quality terms used across the
CWP-700 Composite Wing Panel Production Program suite.
	AS9100
	The aerospace industry's quality management system standard — ISO 9001 plus aviation/space/defense-specific requirements (configuration control, FAI, special-process controls, traceability, counterfeit-parts prevention).

	AS9102
	The specific AS-series standard governing First Article Inspection reporting — the Form 1/2/3 package format.

	First Article Inspection (FAI)
	Full dimensional, material, and process verification of the first production unit of a part before volume production is authorized.

	Material Review Board (MRB)
	The cross-functional board that dispositions nonconforming parts or lots as use-as-is, rework, scrap, or return-to-supplier.

	PPAP
	Production Part Approval Process — supplier-quality qualification process (borrowed from automotive, used in aerospace supply chains) confirming a supplier can reliably produce a part to spec.

	NDT
	Non-Destructive Testing — inspection methods (ultrasonic, X-ray, etc.) that verify internal part integrity without damaging the part.

	Nonconformance
	A part or lot characteristic found not to meet its engineering requirement — the trigger for an MRB disposition.

	Source Inspection
	Customer (OEM) quality representative inspection/witness performed at the supplier's facility, as opposed to at the customer's receiving dock.

	Tier 1 Supplier
	A supplier delivering directly to an aircraft OEM (as opposed to a Tier 2/3 supplier delivering to another supplier).

	Use-as-is
	An MRB disposition accepting a nonconforming part without rework, based on an engineering judgment that it still meets design intent.



